Long delay-line limit interface boxby S�bastien Morel,October 1999

To NS delay-lineTo W delay-line

To computer

+5 VGndPower supply

NS couplersW couplers

To external

PCB organization

External viewTo external

Sub-D connectors

5 4 3 2 19 8 7 6Female (delay-lines)

1 2 3 4 56 7 8 9Male (computer)

Coupler

+5 V1 KW330 W1N914

+5 V fromLimit signal from delay-lineLimit signalto computer

Connector pinoutPin #To NS delay-lineTo W delay-lineTo computer123456789Home (in)Lim + (in)Lim - (in)n.c.n.c.Motor off (out)n.c.n.c.+5 V tank (in)Home (in)Lim + (in)Lim - (in)n.c.n.c.Motor off (out)n.c.n.c.+5 V tank (in)Lim + W (out)Home W (out)Lim + NS (out)Home NS (out)Lim - NS (out)Lim - W (out)Motor off NS (in)Motor off W (in)Gnd(design by Ch. Coldwell)