supply110 V

15 V

20 mA

I2.4 V

Green (on)DB 2511, 9, 7,5,3,1

IStar-tracker piezo transmitter

Equivalent star-trackeramplifier input75 W

I=0 if amplifierplugged inNote: The piezo transmitter contains six identical circuits as described above. The pin-outfor the connectors is respectively for channels 0,1,2,3,4,5.

6142537DIN female output pin-out2 Gnd4 Signal channel 2*n5 Signal channel 2*n+16 DAC common7 DAC commonn =Telescope number (0=North, 1=South, 2=West)Drawing by S�bastien Morel, August 2000