A= Alignment telescope stationB= Star-tracker pick-up mirrorC= Star-tracker CCDD= Star=tracker lensE= BeamsplitterF= Scanning piezo mirrorG= Alignment laserH= Laser beam expanderJ= DiaphragmK= 3-position shutter (delayed open, fixed open, both open)L= Flipping mirrorM= Overlap CCD + baffleN= Green filterP= APD lensR= Avalanche photodiodeS= Flat mirror ft0123456789

10G0123

AHEFFixedbeamDelayedbeamReferencebeam

BCDJKLSNPRMIOTA Visible Table LayoutBy S�bastien Morel, October 2000

= Bolt

01234567890123