(x,y) = (slot,conn,letter; slot, conn,letter)Note: N-Feed, S-Feed, andall Piezo blocks areDC Motor ctrl = NRC boxyou no longer have to manuallyhelp piezo block.Alignment Map & Pico MotorsTel. A FixedTel. B Delay 1Tel. C Delay 2Dec 2002Mirror (x,y)LD1 (laser hut) 21A, 22ALD2 ( laser hut) 21B, 22BExit - Fixed 41A, 42AExit - Delay 1 41B, 42BExit - Delay 2 41C, 42CCorner A 43A, 44ACorner B 43B, 44BCorner C 43C, 44CFeed C 51A, 51B

CWestPiezoNorth FeedCorner A(43A,44A)

Exit fixed (41A, 42A)Fixed Target

Laser1(21A,22A)

SD1LD1yaw

Corner B(43B, 44B)South PiezoBSouthFeed

Exit delay 1 (41B, 42B) fixed - to A delay1 - to B delay2 - to C

Delayed Target

Laser2(21B,22B)

View from Visible Table

South Delayed Case(Newport x,y)

F D1 D2A B C

!Before moving the pico-motors,Make sure the drawing matches the currentconfig. (either South delayed or North Delayed)45’s

Exit delay 2 (41C, 42C)CFeed(51A,51B)

ANorth Piezo

Corner C(43C,44C)(x,y) = (slot,conn,letter; slot, conn,letter)

SD2LED’s in middle of targets andaround feeds.

LD2 yaw

StarTrackerCCDSD1 Yaw 12BSD2 Yaw 12C

Alignment Map & Pico MotorsTel. A Delay 1Tel. B FixedTel. C Delay 2Dec 2002Mirror (x,y)LD1 (laser hut) 21A, 22ALD2 ( laser hut) 21B, 22BExit - Fixed 41A, 42AExit - Delay 1 41B, 42BExit - Delay 2 41C, 42CCorner A 43A, 44ACorner B 43B, 44BCorner C 43C, 44CFeed C 51A, 51B

CWestPiezoNorth FeedCorner A(43A,44A)

Exit fixed (41A, 42A)Fixed Target

Laser1(21A,22A)

SD1LD1yaw

Corner B(43B, 44B)South PiezoBSouthFeed

Exit delay 1 (41B, 42B) fixed - to B delay1 - to A delay2 - to C

Delayed Target

Laser2(21B,22B)

View from Visible Table

North Delayed Case(Newport x,y)

F D1 D2B A C

!Before moving the pico-motors,Make sure the drawing matches the currentconfig. (either South delayed or North Delayed)45’s

Exit delay 2 (41C, 42C)CFeed(51A,51B)

ANorth Piezo

Corner C(43C,44C)(x,y) = (slot,conn,letter; slot, conn,letter)StarTrackerCCDSD1 Yaw 12BSD2 Yaw 12C